<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.3">
<drawing>
<library>
<description>&lt;b&gt; ISD 1700 series chip-corder&lt;/b&gt;&lt;p&gt;
&lt;big&gt;Nuvoton&lt;/big&gt;&lt;br&gt;
&lt;i&gt;&lt;/i&gt;&lt;p&gt;
Created : 2009-04-04 Patrice Nadeau&lt;br&gt;
Modified : 2012-10-24 Patrice Nadeau&lt;br&gt;
&lt;hr&gt;
Copyright (c) 2009, 2010, 2011, 2012 Patrice Nadeau
All rights reserved.&lt;br&gt;
&lt;br&gt;
Redistribution and use in source and binary forms, with or without
modification, are permitted provided that the following conditions are met:&lt;br&gt;
    - Redistributions of source code must retain the above copyright
      notice, this list of conditions and the following disclaimer.&lt;br&gt;
    - Redistributions in binary form must reproduce the above copyright
      notice, this list of conditions and the following disclaimer in the
      documentation and/or other materials provided with the distribution.&lt;br&gt;
    - Neither the name of Patrice Nadeau nor the names of its contributors 
	  may be used to endorse or promote products derived from this software 
      without specific prior written permission.&lt;br&gt;
&lt;br&gt;
THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS IS" AND
ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED
WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE
DISCLAIMED. IN NO EVENT SHALL Patrice Nadeau BE LIABLE FOR ANY
DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES
(INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES;
LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND
ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT
(INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS
SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.</description>
<packages>
<package name="DIP-28_LARGE">
</package>
<package name="POWER">
</package>
</packages>
<symbols>
<symbol name="ISD1740">
<pin name="VCCD" direction="pwr"/>
<pin name="!LED" direction="out" function="dot"/>
<pin name="!RESET" direction="in" function="dot"/>
<pin name="MISO"/>
<pin name="MOSI"/>
<pin name="SCLK" direction="in"/>
<pin name="!SS" direction="in" function="dot"/>
<pin name="VSSA" direction="sup"/>
<pin name="ANAIN" direction="in"/>
<pin name="MIC+" direction="in"/>
<pin name="MIC-" direction="in"/>
<pin name="VSSP2" direction="sup"/>
<pin name="SP-" direction="out"/>
<pin name="VCCP" direction="pwr"/>
<pin name="VSSD" direction="sup"/>
<pin name="!INT!/RDY" direction="in"/>
<pin name="!FWD" direction="in" function="dot"/>
<pin name="!ERASE" direction="in" function="dot"/>
<pin name="!REC" direction="in" function="dot"/>
<pin name="!PLAY" direction="in" function="dot"/>
<pin name="!FT" direction="in" function="dot"/>
<pin name="VCCA" direction="pwr"/>
<pin name="ROSC" direction="in"/>
<pin name="!VOL" direction="in" function="dot"/>
<pin name="AGC" direction="in"/>
<pin name="AUD/AUX" direction="out"/>
<pin name="VSSP1" direction="sup"/>
<pin name="SP+" direction="out"/>
</symbol>
<symbol name="ISD1700">
<pin name="!REC" direction="in" function="dot"/>
<pin name="!PLAY" direction="in" function="dot"/>
<pin name="!ERASE" direction="in" function="dot"/>
<pin name="!FWD" direction="in" function="dot"/>
<pin name="!VOL" direction="in" function="dot"/>
<pin name="!FT" direction="in" function="dot"/>
<pin name="!SS" direction="in" function="dot"/>
<pin name="SCLK" direction="in"/>
<pin name="MOSI"/>
<pin name="MISO"/>
<pin name="MIC+" direction="out"/>
<pin name="MIC-" direction="out"/>
<pin name="ANAIN" direction="in"/>
<pin name="ROSC" direction="in"/>
<pin name="AGC" direction="in"/>
<pin name="!RESET" direction="in" function="dot"/>
<pin name="!LED" direction="out" function="dot"/>
<pin name="VCCD" direction="pwr"/>
<pin name="VSSD" direction="sup"/>
<pin name="VCCA" direction="pwr"/>
<pin name="VSSA" direction="sup"/>
<pin name="VCCP" direction="pwr"/>
<pin name="VSSP1" direction="sup"/>
<pin name="VSSP2" direction="sup"/>
<pin name="SP+" direction="out"/>
<pin name="SP-" direction="out"/>
<pin name="AUD/AUX" direction="out"/>
<pin name="!INT!/RDY" direction="in"/>
</symbol>
<symbol name="VCCD">
<pin name="VCCD" direction="pwr"/>
</symbol>
<symbol name="VCCA">
<pin name="VCCA" direction="pwr"/>
</symbol>
<symbol name="VCCP">
<pin name="VCCP" direction="pwr"/>
</symbol>
<symbol name="GND_ANALOG">
<pin name="GND_ANALOG" direction="sup"/>
</symbol>
<symbol name="GND_DIGITAL">
<pin name="GND_DIGITAL" direction="sup"/>
</symbol>
<symbol name="GND_SP+">
<pin name="GND_SP+" direction="sup"/>
</symbol>
<symbol name="GND_SP-">
<pin name="GND_SP-" direction="sup"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="ISD1700">
<description>Winbound ISD 1700 series voice recorder&lt;p&gt;

Patrice Nadeau 2009-04-04&lt;br&gt;
&lt;hr&gt;
Use the included power and gnd symbols to separate the power and grounds as the datasheet.</description>
<gates>
<gate name="G$1" symbol="ISD1700"/>
</gates>
<devices>
<device name="" package="DIP-28_LARGE">
<connects>
<connect gate="G$1" pin="!ERASE" pad="25"/>
<connect gate="G$1" pin="!FT" pad="22"/>
<connect gate="G$1" pin="!FWD" pad="26"/>
<connect gate="G$1" pin="!INT!/RDY" pad="27"/>
<connect gate="G$1" pin="!LED" pad="2"/>
<connect gate="G$1" pin="!PLAY" pad="23"/>
<connect gate="G$1" pin="!REC" pad="24"/>
<connect gate="G$1" pin="!RESET" pad="3"/>
<connect gate="G$1" pin="!SS" pad="7"/>
<connect gate="G$1" pin="!VOL" pad="19"/>
<connect gate="G$1" pin="AGC" pad="18"/>
<connect gate="G$1" pin="ANAIN" pad="9"/>
<connect gate="G$1" pin="AUD/AUX" pad="17"/>
<connect gate="G$1" pin="MIC+" pad="10"/>
<connect gate="G$1" pin="MIC-" pad="11"/>
<connect gate="G$1" pin="MISO" pad="4"/>
<connect gate="G$1" pin="MOSI" pad="5"/>
<connect gate="G$1" pin="ROSC" pad="20"/>
<connect gate="G$1" pin="SCLK" pad="6"/>
<connect gate="G$1" pin="SP+" pad="15"/>
<connect gate="G$1" pin="SP-" pad="13"/>
<connect gate="G$1" pin="VCCA" pad="21"/>
<connect gate="G$1" pin="VCCD" pad="1"/>
<connect gate="G$1" pin="VCCP" pad="14"/>
<connect gate="G$1" pin="VSSA" pad="8"/>
<connect gate="G$1" pin="VSSD" pad="28"/>
<connect gate="G$1" pin="VSSP1" pad="16"/>
<connect gate="G$1" pin="VSSP2" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VCCD">
<gates>
<gate name="G$1" symbol="VCCD"/>
</gates>
<devices>
<device name="" package="POWER">
<connects>
<connect gate="G$1" pin="VCCD" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VCCA">
<gates>
<gate name="G$1" symbol="VCCA"/>
</gates>
<devices>
<device name="" package="POWER">
<connects>
<connect gate="G$1" pin="VCCA" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VCCP">
<gates>
<gate name="G$1" symbol="VCCP"/>
</gates>
<devices>
<device name="" package="POWER">
<connects>
<connect gate="G$1" pin="VCCP" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GND_ANALOG">
<gates>
<gate name="G$1" symbol="GND_ANALOG"/>
</gates>
<devices>
<device name="" package="POWER">
<connects>
<connect gate="G$1" pin="GND_ANALOG" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GND_DIGITAL">
<gates>
<gate name="G$1" symbol="GND_DIGITAL"/>
</gates>
<devices>
<device name="" package="POWER">
<connects>
<connect gate="G$1" pin="GND_DIGITAL" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GND_SP-">
<gates>
<gate name="G$1" symbol="GND_SP-"/>
</gates>
<devices>
<device name="" package="POWER">
<connects>
<connect gate="G$1" pin="GND_SP-" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GND_SP+">
<gates>
<gate name="G$1" symbol="GND_SP+"/>
</gates>
<devices>
<device name="" package="POWER">
<connects>
<connect gate="G$1" pin="GND_SP+" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
